Environment

This script is only developed for Windows platform

Installation

The setup files can be found at the link below:

1. Double click "python-2.7.6.msi" to install

2. Double click "pyserial-2.7.win32.exe" to install COM port library

HA Controller Firmware

The firmware is located at the link below:

ftp:192.168.8.16/Project/uZiP/Atmel/SW Release/v0.3.00\_00.16.0x/uZiP\_Atmel\_HAcontroller\_v0.3.00\_00.16.00\_UART0\_R50\_D6\_C30\_ED25.hex

How to use

1. Ensure the device is factory new

2. Open 'Script' folder

3. Check the COM port number in control panel

4. Open 'serialConfig.py' and make sure the COM port number is correct

5. Run 'getDeviceInfo.py' and wait until complete

6. Open 'log' folder

7. Open 'deviceInfo.txt' to view the device info